EXPRESSION OF INTEREST (EOI)

**EOI Reference #: ASMC-WRTI-EOI-2023-006**

**Title: SE818 – Marine Rigging and Equipment**

**Project: West White Rose CGS Tow-out & Installation**

**Issue Date:** April 19, 2023

**Closing Date:** May 3, 2023

**GENERAL**

Aker Solutions Marine Contractors Limited (ASMC) hereby invites interested parties to submit an Expression of Interest (EOI) related to the future Requests for Tender for the following Scope of Work in connection with ASMC CGS Tow-out and Installation Scope of Work for the Cenovus West White Rose Project in Newfoundland and Labrador, Canada.

**BENEFITS COMMITMENTS**

ASMC is committed to providing full and fair opportunities to commercially competitive Canadian companies with first consideration given to those from Newfoundland and Labrador. At the Pre-Qualification and ITT stages, companies will be required to complete Canada/Newfoundland & Labrador Benefits questionnaires to acknowledge their willingness to comply with the White Rose Canada-Newfoundland and Labrador Benefits Plan.

**EQUAL OPPORTUNITY**

ASMC is an equal opportunity employer and supports diversity in the workplace. Successful suppliers and subcontractors to ASMC will be required to undertake a commitment to support diversity in execution of work on the West White Rose Project.

**SCOPE OF SERVICES**

It is intended that Frame Agreements will be established with one or more vendors. The establishment of Frame Agreements with one or more vendors does not guarantee a Purchase Order. Equipment orders will be placed via subsequent Requests for Quotation (RFQ) from each vendor as the need arises. Scope of supply requirements may include, but not be limited to the following:

* Lifting container with closable lid, certified to DNV 2.7-1 (dimensions not to exceed (LxWxH) 3.5 m L x 2.0 m W x 1.7 m H) (TBC). Container shall be supplied with DNV 2.7-1 certified wire rope lifting bridle.\*
* Heavy duty, puncture-tear-cut resistant lifting bag with closable top and integrated lifting straps/slings.\* Max gross weight not to exceed 6 Te.
* Lifting bags with closable top (e.g. draw string, zipper, or other suitable means), SWL 75 kg. Bag foot-print/diameter not to exceed 0.6 m L x 0.6 m W, or 0.6 m in diameter, when full.
* Small hand tools:
	+ Combination wrench sets (SAE (1/8” to 2.5”, and or metric (3 mm to 30 mm))
	+ Socket set with ratchet wrenches (1/4”, ½”, ¾” drive)
	+ Impact wrench (1/2” and ¾” drive, minimum 8.5A, corded or cordless (24V))
	+ Screwdrivers
	+ Pliers
	+ Etc.
* Wire Rope Sling: 6 x 26 galvanized EIPS IWRC, (diameters vary from 16mm to 25mm, lengths vary from 1m to 25m) c/w Crosby G-414 Standard or Extra Heavy Thimble each end\*
* Crosby Bolt Type Anchor Shackle (capacities vary from 3.25Te to 25.0Te, G-2130) or an approved equivalent \*
* Endless loop synthetic slings (lengths varying from 1 m to 3 m, 1Te to 5 Te WLL).
* Wire Rope Equal and unequal four-legged bridle assemblies: 25mm dia, length 3m, 6 x 26 galvanized EIPS IWRC with Crosby G-414 Extra Heavy thimble come with Crosby A-345CT 44W dia. master link assembly or an approved equivalent\*
* Wire Rope Equal two-legged bridle: 19mm dia, length 5m, 6 x 26 galvanized EIPS IWRC with Crosby G-414 Extra Heavy thimble c/w Crosby A-345 22W dia. master link assembly or an approved equivalent\*
* Crosby A-342 Masterlinks with varying diameters or an approved equivalent\*
* Electric chain hoist, 208 V, 3 phase, 60 Hz, 5 Te WLL\*
* Other miscellaneous rigging

\* shall comply with ‘CAPP Code of Practice - Safe Lifting Practice Respecting Design Operation & Maintenance of Materials Handling Equipment’ and applicable ASME codes.

Note: Wire rope slings/bridles may require load testing, and applicable documentation demonstrating proof of testing to be submitted for review.

**SCHEDULE AND DELIVERY**

**Required On Site date (Tentative): March 15, 2024**

Delivery Location: CGS Construction Site at Argentia, NL

**SUBMISSION REQUIREMENTS**

As part of the submission requirements, suppliers are requested to provide Aker Solutions Marine Contractors Limited with the following answers and/or information:

1. Please provide a brief outline of the following company information:
	1. Copy of Certificate of Incorporation.
	2. Company Name and Address.
	3. Single Point of Contact, c/w contact details.
2. A list of previous work experience related directly to the scope of services including supply, testing and certification of rigging suitable for use in a marine environment as well as relevant experience coordinating third-party certification e.g., DNV, CSA, etc. This list should include but not be limited to the client’s name, project date, location, specific industry sector and proposed manufacturer.
3. Overview of your company’s equipment and tools maintenance and calibration/recertification program with specific reference to the database being used to manage this.
4. Please provide a brief description and overview of the execution plan, facility(ies) being proposed to execute the work, and sub-supplier(s). Also, please provide details related to work that will be subcontracted (if any) and outline the expected scopes and subcontractor options (names and locations).
5. If available, please provide catalogues of equipment included in regular inventory, and indicative lead times for items not kept in stock.

6. Company shall demonstrate familiarity with CAPP Safe Lifting Practice and AMSE codes applicable to lifting and rigging equipment.

**RESPONSE REQUIREMENTS**

Suppliers are to respond to the following e-mail address: ASMC.WRTI\_Procurement@akersolutions.com

on or before the closing date noted above.

The subject line of the email must contain the following:

**EOI REFERNCE NUMBER – TITLE – Supplier Company Name**

Suppliers that have not been pre-qualified will be required to do so before the formal RFQ/Tender/Bid packages.

If you have any questions regarding this announcement, please contact Aker Solutions Single Point of Contact listed below:

Tanya O’Neill

Contracts Manager

Aker Solutions Marine Contractors Limited

tanya.oneill@akersolutions.com